cenrep
version 1 # refers to the version of the file-format, not of this file

[owner]
0x200269A5

[defaultmeta]
16777216
 
[platsec]
cap_rd=alwayspass cap_wr=WriteDeviceData
 
[Main]

#
#   TCP-CIR Settings Group  0x01------
#

# TCP-CIR protol version number
0x01000000 int 1 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# Snap id
# Change the snap-id to configurable id for emulator.
#0x01000001 int <snap-id> 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData 

# IAP id
# Change the iap-id to configurable id for emulator.
#0x01000002 int <iap-id> 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData 

# TCP-CIR gateway address
0x01000003 string "207.245.49.36" 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR gateway port
0x01000004 int 8008 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR ping minimum ##s
0x01000005 int 180 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR ping maximum ##s
0x01000006 int 1800 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR ping increment ##%
0x01000007 int 10 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR ping decrement ##%
0x01000008 int 50 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR ping start ##s
0x01000009 int 900 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR ping interval increase delay ##s
0x0100000A int 86400 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR ping last success
0x0100000B int 0 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR WLAN ping minimum ##s
0x0100000C int 60 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR WLAN ping maximum ##s
0x0100000D int 1800 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR WLAN ping increment ##%
0x0100000E int 10 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR WLAN ping decrement ##%
0x0100000F int 50 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR WLAN ping start ##s
0x01000010 int 1200 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR WLAN ping interval increase delay ##s
0x01000011 int 86400 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR WLAN ping last success
0x01000012 int 0 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR ping reconnect count
0x01000013 int 5 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR ping reconnect interval
0x01000014 int 7200 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

# TCP-CIR Gateway Protocol
0x01000015 string "cir" 16777216 cap_rd=alwayspass cap_wr=WriteDeviceData

