cenrep
version 1 # versio
[owner]
0x20000907 # app UID
[defaultmeta]
 16777216 # (0x01000000) = backup
[platsec]
cap_rd = ReadDeviceData cap_wr = WriteDeviceData  # read & write access
[Main]
# id     type   value    backup? (use 16777216) cap_rd 			cap_rw   
#----------------------------------------------------------------------------------------------------------------------------
0x00     int     1       0			cap_rd=ReadDeviceData 	cap_wr=WriteDeviceData # Settings Have Changed (boolean)
0x01     int     -1      16777216 		cap_rd=ReadDeviceData 	cap_wr=WriteDeviceData # Accesspoint
0x02     int     -1      16777216 		cap_rd=ReadDeviceData 	cap_wr=WriteDeviceData # Network permission
0x03	 int	 0	 16777216 		cap_rd=ReadDeviceData 	cap_wr=WriteDeviceData # Number of installed plugin updates so far
0x04	 int	 0	 16777216 		cap_rd=ReadDeviceData 	cap_wr=WriteDeviceData # Default local search plugin (deprecated)
0x05	 int	 0	 16777216 		cap_rd=ReadDeviceData 	cap_wr=WriteDeviceData # Default maps search plugin (deprecated)
0x06	 int	 1	 16777216 		cap_rd=ReadDeviceData 	cap_wr=WriteDeviceData # Show Tooltips
0x07     string  "達 " 	 16777216 		cap_rd=ReadDeviceData 	cap_wr=WriteDeviceData # Disabled AIS plugins. UIDs are binarycoded in reversed byte order. Use hex-editor to edit.
0x08     int     1       16777216		cap_rd=ReadDeviceData 	cap_wr=WriteDeviceData # Clear search history (1 to clear on next startup)
0x09     int     0       16777216               cap_rd=ReadDeviceData 	cap_wr=WriteDeviceData # First startup
0x0a     int     0       16777216               cap_rd=ReadDeviceData 	cap_wr=WriteDeviceData # Selected country countrycode
0x0b     string  ""      16777216               cap_rd=ReadDeviceData 	cap_wr=WriteDeviceData # Binary format list of prefered providers
0x0c     string  ""      16777216               cap_rd=ReadDeviceData 	cap_wr=WriteDeviceData # Disabled plugins
0x0d     int     0       16777216                cap_rd=ReadDeviceData cap_wr=WriteDeviceData # ISLite integration: Default provider UID
0x0e     int     0       16777216                cap_rd=ReadDeviceData cap_wr=WriteDeviceData # ISLite integration: Application ID who has set the default provider
0x0f     string  ""      16777216                cap_rd=ReadDeviceData cap_wr=WriteDeviceData  # SHA1 id code
